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Paper Pad Machine
Model: P300HD
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Introduction:
After being folded by the P300HD machine, rolled in the middle, and crimped on the sides, Kraft paper forms a 3D cushion with numerous small cavities, offering excellent support and cushioning effects. The length of the cushion can be adjusted as needed. When coiled into a disk shape, its compressive strength and elasticity are sufficient to bear the weight of heavy items up to 60 kg. The versatile packaging methods not only provide filling, cushioning, and wrapping functions but also secure items to reduce shaking, thereby avoiding increased costs due to product damage.    

Features: 
1. Multi-language Interface: Supports operation panels in 12 preset languages.  

2. Customized Output: Allows adjustment of length and quantity based on needs.  

3. Three Simple Modes: Offers user-friendly operation with three distinct modes.  

4. Operation Modes:  

   (a) Continuous Auto-feed: Uninterrupted paper output.  

   (b) Take-One-Replenish-One: Automatically replaces each dispensed unit.  

   (c) Foot Pedal Control: Manual control via pedal for flexible packaging demands.  

5. Robust Construction: Durable iron-shell exterior design.  

6. Modular System: Easy blade replacement and maintenance with modular components.  




Specification:

	Model
	P300HD

	Speed
	27m/min

	Acceptable paper type
	Triple-fold Roll Paper

	Operation
	Complement/Automatic/Pedal

	Power
	230W

	Voltage
	30V,100V/50/60H

	Weight
	100kgs

	Size
	934*597*1358mm


Acceptable paper type:
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